 ***New F510 PRO*** 

 ***Meyer Formula Vertical*** *TMR* ***Mixer***

**Model *F510 PRO* - offering 510-570 Cubic Foot Capacity**

 ***Formula Premium Single Screw Vertical Mixer***

 **Same extensive line of conveyor options as the popular twin screw models**

**Front Door & Side Door Versions offering our popular belt conveyor systems to eliminate carryback & noise while maximizing feed delivery performance!**

NEW!

 ** **

**Front Door or Side Door *- F510 PRO Our popular belt incline conveyor***

 **Belt or Chain Conveyors Available Unloads off Either the Incline or Flat Side**

 **Viewing Platform Optional on Front Door Models Belt Capacity Ext (pictured) or Hay Retention avail**

**Meyer F510 PRO-Upgraded to meet the needs of your livestock operation**

 *** ***

 ***40 Max RPM Auger Speed for Fast Cleanout The PRO Series – HD Frame/Axle***

***Magnet options: kicker arm, tank, deflector & more Premium Floatation & Ride***

***Unique, Sectional knife system / auger kicker arm with Uncompromised Strength***

***STANDARD FEATURES OF THE F510 PRO:***

***1000 RPM Direct Drive, Shear-Bolt Protection, Upgraded - HD VM10 Planetary Drive System***

 ***Cone Center Augers w/Adj Lead Edge Scraper / High Clearance Design Ideal in Rough Terrain***

***Robust undercarriage w/3 point scale & large diameter tires - Full Line of Scale Head Options***

 ***Phone# 1-800-325-9103 meyermfg.com contact us:*** ***sales@meyermfg.com***